Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 74 - Shawl Weaving Artisan - TP
P. 74

    TASK 5: Drafting process of 2/2 twill weave

           1  Take the 4 heald  shaft and  place  it in front of the   5  Then take the fourth warp thread and draw in through
              warp beam.                                           the first heald eye of the fourth heald shaft.
           2  According to the design, take a first  threads from   6  Likewise draw all the warp threads(e.g)
              warp beam and insert it through the first heald eye of   1 → 2 → 3 → 4 → 1 → 2 → 3 → 4
              the first heald shaft with the help of heald hook.
                                                                1 = First heddle on Shaft 1
           3  Then take the second thread from the beam and
              draw  in through the first heald eye of  the second   2 = First heddle on Shaft 2
              heald shaft.                                      3 = First heddle on Shaft 3
           4  Then take the third warp thread and draw in through   4 = First heddle on Shaft 4
              the first heald eye of the third heald shaft.
                                                                7  Repeat across the width of the warp.

           TASK 6: Denting process of 2/2 twill weave
           1  Take a reed.                                         •  Dent 3: Threads from shafts 1 & 2

           2  Put the heald hook and draw the 2 threads per dent.  •  Dent 4: Threads from shafts 3 & 4
           3  Take first two threads from the heald shafts and draw   4  Likewise draw all the threads
              it in the first dent of the reed e.g.
                                                                5  Repeat across the reed.
              •  Dent 1: Threads from shafts 1 & 2
              •  Dent 2: Threads from shafts 3 & 4

           TASK 7 : Construct satin weave (5 end) (Fig 1)

           1  Take a note book.
                                                                  Fig 1
           2  Draw a 5 × 5 grid (for a 5-end satin repeat).
           3  Set  the Binding Points – Place dots using a satin
             progression of 2:

             •  Row 1: Column 1
             •  Row 2: Column 3
             •  Row 3: Column 5
             •  Row 4: Column 2
             •  Row 5: Column 4

           4  Mark Warp Floats (X), the empty spaces  in each
             row represent warp threads floating over four weft
             threads.
           5  Repeat the Pattern extend the design across the grid
             to form a continuous weave.

           62             Textile & Handloom : Shawl Weaving Artisan (NSQF - 2024) Exercise 1.5.41

| 69 70 71 72 73 74 75 76 77 78 79 |