Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 37 - Shawl Weaving Artisan - TP
P. 37

    Step 5: Start warping operation                       Step 6: Final checks and beam labelling
                •  Start machine slowly.                              •  Stop machine once required length is reached.

                •  Observe yarn winding and tension.                  •  Cut and tie ends.
                •  Pause machine to check alignment  after 100–200    •  Label beam with job details.
                   meters.                                            Beam labelling

                             Trainee observation table
                                                                         S.No.         Detail             Value
                         Observation
                 S.No.                 Status ( /X)   Remarks
                             point                                         1        Yarn count
                         Yarn Winding
                    1                                                      2        No. of Ends
                         Evenly?
                         Any crossed
                    2                                                      3        Warp length
                         ends?
                         Yarn tension
                    3                                                      4        Job number
                         uniform?
                         Machine                                           5        Date
                    4    running
                         smoothly?                                         6        Trainee name

                                Textile & Handloom : Shawl Weaving Artisan (NSQF - 2024) Exercise 1.2.19            25

| 32 33 34 35 36 37 38 39 40 41 42 |