Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 42 - Shawl Weaving Artisan - TP
P. 42

    Textile & Handloom                                                               Exercise 1.2.23

           Shawl Weaving Artisan - Winding and Warping

           Operation of warp and winding machine

           Objectives : At the end of this exercise you shall be able to
           •  perform setting of warping and winding machine.

             Requirements

              Tools/Equipment’s/Instruments
             •  Winding machine                  - 1No.         •   Reed                              - 1No.
             •   Warp drum                       - 1No.         •   Bobbins                           - 1No.
             •   Creel                           - 1No.         •   Measuring tape                    - 1No.
             •   Warping heck                    - 1No.         •   Lease rods                        - 1No.

           PROCEDURE

           A  Start the Winding Machine
              1  Turn on the winding  machine  at a moderate       6  Check for broken ends and fix immediately.
                speed.                                             7  Store wound pirns near the weaving section for

              2  Monitor the yarn supply and ensure uniform           easy access.
                winding onto pirns/bobbins.
                                                                   8  Ensure the warping process finishes in time for
              3  Replace filled pirns/bobbins regularly to maintain   the next loom setup.
                continuous weft supply.
                                                                   9  Clean the  drum surface,  creel, and guides to
           B  Start the Warping Machine                               prevent contamination.
              1  Before starting the warping process, check the    10 Securely fix the empty warp beam onto the
                machine for proper working conditions.                machine.
              2  Begin winding the warp threads onto the warping   Final quality check and maintenance
                drum.
                                                                1  Inspect both warp  and  weft yarns  for tension
              3  Adjust speed to match the required warp length.   uniformity and defects.
              4  Monitor tension and alignment to avoid defects.  2  Clean machines after operation to remove dust and
                                                                   fiber residues.
              5  Adjust winding  and warping speeds based on
                weaving consumption.                            3  Lubricate moving parts to ensure smooth functioning
                                                                   for the next production cycle.

           Textile & Handloom                                                               Exercise 1.2.24
           Shawl Weaving Artisan - Winding and Warping

           Yarn package faults and causes

           Objectives : At the end of this exercise you shall be able to
           •  identify yarn package faults and causes.

             Requirements
              Tools/equipment’s/Instruments

             •  Notebook                         - 1No.         •   Pencil                            - 1No.
             •   Eraser                          - 1No.         •   Sharpener                         - 1No.

           PROCEDURE

                                             Refer exercise No.1.1.06 - Task No 2

           30

| 37 38 39 40 41 42 43 44 45 46 47 |