Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 49 - Shawl Weaving Artisan - TP
P. 49

    Step 4: Check and verify                              Step 2: Mount the harnesses
                1  Check the cut cards for accuracy and precision.    1  Mount the harnesses on  the loom, following  the
                                                                        harness mounting plan.
                2  Verify that the cards match the design and loom
                   requirements.                                      2  Ensure that the harnesses are properly aligned and
                3  Card punching                                        secured.
                                                                      Step 3: Load the cards
                Step 1: Prepare the card punch
                                                                      1  Load the  cut  cards into the  loom’s  card cutting
                1  Ensure the card punch is clean and free of debris.
                                                                        system.
                2  Check the card punch for any damage or wear.
                                                                      2  Ensure that the cards are properly  aligned  and
                Step 2: Align the card                                  secured.
                1  Align the card with the card punch, ensuring proper   5  Weaving
                   registration.
                                                                      Step 1: Start the loom
                2  Check that the card is properly seated in the punch.
                                                                      1  Start  the loom, ensuring that the harnesses and
                Step 3: Punch the card                                  cards are properly aligned.
                1  Use the card punch  to create holes  in the card,   2  Check  that the loom  is operating  smoothly  and
                   following the desired pattern.                       quietly.
                2  Apply gentle to moderate pressure, depending  on   Step 2: Monitor the weave
                   the card material and punch type.
                                                                      1  Monitor the weave, ensuring that the design is being
                Step 4: Verify the punches                              woven correctly.
                1  Verify that the punches are accurate and precise.  2  Check for any errors or defects in the weave.
                2  Check that the holes are correctly placed and sized.  Step 3: Adjust as needed
                4  Loom preparation                                   1  Adjust the loom as needed to ensure proper weaving.

                Step 1: Thread the loom                               2  Check that  the harnesses and cards are properly
                1  Thread the  loom with the warp yarns,  ensuring      aligned and secured.
                   proper tension and alignment.

                2  Check that the warp yarns are evenly spaced and
                   properly secured.

                                Textile & Handloom : Shawl Weaving Artisan (NSQF - 2024) Exercise 1.3.29            37

| 44 45 46 47 48 49 50 51 52 53 54 |