Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 68 - Shawl Weaving Artisan - TP
P. 68

    Table 2                                              Table 3

            S.No.       Parameter              Value             S. No.        Parameter              Value
              1     Total Ends          2400                       1    Total ends required            3600
              2     Ends per inch (EPI)  60                        2    EPI                             80
              3     Width of warp       40 inches                                                     1 inch
              4     Section width       1 inch                     3    Section width
              5     Number of sections  40                         4    Warp beam flange width       60 inches
              6     Ends per section    60                         5    Creel capacity              120 cones
              7     Creel capacity      100 cones/ bobbins      b  Calculate the given data (Table 4)
              8     Patterns per section  1                                          Table 4
           7  Analysis                                                                               Students
                                                                 S. No.         Parameter
              •  Warp width is within beam flange width (Beam                                           data
                flange = 50 inches, warp width = 40 inches).
                                                                   1       Total ends
              •  Creel capacity is sufficient for this warp plan.
                                                                   2       EPI
              •  Only 1 loading pattern per section is required.
                                                                   3       Warp width
              •  No  extra  creel changeover  needed during
                warping.                                           4       Section width
           8  Practical worksheet for trainees                     5       Number of sections
              a  Given data (Table 3)                              6       Ends per section

                                                                   7       Creel capacity
                                                                   8       Patterns per section

                                                                   9       Total ends

           56             Textile & Handloom : Shawl Weaving Artisan (NSQF - 2024) Exercise 1.4.38

| 63 64 65 66 67 68 69 70 71 72 73 |