Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 27 - Shawl Weaving Artisan - TP
P. 27

    TASK 3: Starting and stopping of pirn winder

                Starting the machine                                  Stopping the machine
                1  Ensure the machine is clean, properly maintained,   1  Press the stop button to halt the winding process.
                   and all components are in place.
                                                                      2  Check the pirn to ensure it is fully wound and yarn is
                2  Check the yarn path, tensioners, guides,  and the    evenly distributed.
                   pirn to ensure everything is set up correctly.
                                                                      3  Cut the yarn close to the pirn.
                3  Secure the pirn onto the winding spindle.          4  Remove the pirn off carefully from the spindle without

                4  Thread the yarn through the guides and secure it to   damaging the wound yarn.
                   the pirn.
                                                                      5  Remove any yarn waste or lint from the spindle and
                5  Switch on the main power supply of the machine.      surrounding areas.
                6  Adjust the speed,  tension, and  traverse settings   6  Prepare the machine for the next operation.
                   based  on the yarn type and  desired  winding
                   requirements.

                7  Press the start button to initiate the winding process.
                8  Monitor the machine for smooth operation and even
                   winding.

                                Textile & Handloom : Shawl Weaving Artisan (NSQF - 2024) Exercise 1.2.12            15

| 22 23 24 25 26 27 28 29 30 31 32 |