Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 52 - Shawl Weaving Artisan - TP
P. 52

    15

               16

            TASK 2: Operate fly shuttle loom for weaving

           1  Mount the heald frames in the fly shuttle loom.
                                                                  Fig 1
           2  Connect the top portion of the heddles at the top of
              the fly shuttle loom.

           3  Connect the bottom portion of the heddles  to the
              treadles/pedals.
           4  Connect the four heald shafts with the four treadles.
              as shown in Fig 1
           5  Now press the first pedal and observe the movement
              of heald frame.

           6  Then press the second pedal to bring the heddles
              down.
           7  Likewise operate all the pedals.

           TASK 3: Operate through shuttle loom for weaving
           1  Mount the heald frames in the through shuttle loom   Fig 1
              with the help of cords.
           2  Connect the top portion of the heddles to the jacks
              which is placed at the top of the through shuttle loom
              with the help of cords.
           3  Connect the bottom portion of the heddles with lam
              rods.
           4  Now connect the  lam rods with the  treadles.as
              shown in Fig 1.

           5  Now press the first pedal and observe the movement
              of heald frame.

           40             Textile & Handloom : Shawl Weaving Artisan (NSQF - 2024) Exercise 1.3.30

| 47 48 49 50 51 52 53 54 55 56 57 |