Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 65 - Shawl Weaving Artisan - TP
P. 65

    7  Move the reed frame towards the front centre. This   Fig 3
                   action is beat up. At this time move the reed slightly
                   at higher force. As shown in Fig 3
                8  The beat up force must be uniform for all the weft
                   threads.
                9  Repeat the process.

                TASK 6: Drafting process in through shuttle loom

                1  Draft the warp yarns as mentioned in task 1.

                TASK 7: Denting process in through shuttle loom
                1  Denting process is same as mentioned in task .2.

                TASK 8: Inserting pirn into the shuttle

                1  Take a shuttle (small  in size) which  is used  in   5  Now take the thread from the pirn and pass it through
                   traditional through shuttle loom.                    the eye in the shuttle.
                2   Check the shuttle against any damage.             6  Pull the length of the yarn from the pirn. (Fig 2)

                3   Take the full pirn and place it into the shuttle.  Fig 2
                4  Fix the pirn perfectly into the shuttle. (Fig 1)
                  Fig 1

                TASK 9: Weave the plain shawl on the through shuttle loom

                1  Press the treadles by using legs to raise the healds   Fig 1
                   up and down.

                2  Now the warp threads will divide in two layers to form
                   a shed.
                3  Pull the shuttle between the shed with the help of
                   hand i.e.(right hand to left hand). (Fig 1)

                                Textile & Handloom : Shawl Weaving Artisan (NSQF - 2024) Exercise 1.4.37            53

| 60 61 62 63 64 65 66 67 68 69 70 |