Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 25 - Shawl Weaving Artisan - TP
P. 25

    Textile & Handloom                                                                Exercise 1.2.11

                Shawl Weaving Artisan - Winding and Warping

                Winding of pirn from cone

                Objectives : At the end of this exercise you shall be able to
                •  prepare a pirn from cone bobbin for weaving process.

                  Requirements
                   Tools/equipment’s/Instruments                      Materials

                   •  Pirn winding machine             - 1 No.        •  Cone bobbin                        - 1 No.
                   •  Empty Pirn                       - as reqd.

                PROCEDURE

                TASK 1 : Prepare pirn from cone

                1  Take an empty pirn and place it in the spindle of the
                   pirn winding machine.                              Fig 3
                2  Place the cone bobbin  near to the pirn winding
                   machine. (Fig 1)
                 Fig 1

                                                                       Fig 4

                3  Take the end of the thread from cone  bobbin  and
                   hold it against the pirn with your finger. (Fig 2)

                 Fig 2                                                 Fig 5

                                                                      8  Remove  the pirn  from the spindle  of pirn  winding
                                                                        machine. (Fig 6)

                                                                       Fig 6
                4  Start the pirn winding machine and keep the speed
                   slow.
                5  With the help of one hand guide the yarn to the pirn.
                   (Fig 3 & 4)
                6  Start the winding process from base of the pirn and
                   slowly move to the tip of the pirn. (Fig 5)
                7  After completing the winding process switch off the
                   pirn winding machine.
                                                                      9  Now insert the other empty  pirn and start the process

                                                                                                                    13

| 20 21 22 23 24 25 26 27 28 29 30 |