Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 30 - Shawl Weaving Artisan - TP
P. 30

    Textile & Handloom                                                               Exercise 1.2.15

           Shawl Weaving Artisan - Winding and Warping

           warp making process and formation of stripe design and color

           Objectives : At the end of this exercise you shall be able to
           •  set up bobbins on a creel
           •  create colourful stripe patterns while doing drum warping.

             Requirements

              Tools/Equipment’s/Instruments
              •  Creel                          - 1 No.         •  Scissor small size                 - 1 No.
              •  Bobbins                        - 1 No.         •  Color pencils                      - 1 Set.
              •  Warping drum                   - 1 No.         Materials
              •  Graph paper                    - as reqd.
              •  Measuring tape                 - as reqd.      •  Yarn samples in bobbin
                                                                     3 or more coloured yarn cones
                                                                   (Red, Blue, Yellow, etc.)          - 200

           PROCEDURE

           TASK 1 : Set up bobbins on the creel
           1  Clean the  creel and place it  near to  the  warping
              drum.                                              Fig 2
           2  Inspect the bobbin for any defects or damage.
           3  Choose the  correct bobbin type and size for  the
              creel.
           4  Stand in front of the creel and locate the appropriate
              spindle (peg) for the bobbin.

           5  Hold the bobbin firmly with both hands.
           6  Place bobbins in the creel in the correct order for
              warping. (Fig 1)

           Fig 1

                                                                8  Guide it through the tensioning devices.
                                                                9  Observe proper threading according to the specific
                                                                   creel setup to maintain tension and alignment.

                                                                10 Observe the thread feeds smoothly from the bobbin.
                                                                11 Repeat the process for each bobbin.
                                                                12 Inspect all  bobbins  to ensure  they are securely
                                                                   mounted and properly threaded.
                                                                13 Once all bobbins are in place and the creel is properly
                                                                   set up, start the operation.
           7  Pull the yarn from the bobbin’s end. (Fig 2)

           18

| 25 26 27 28 29 30 31 32 33 34 35 |