Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 38 - Shawl Weaving Artisan - TP
P. 38

    Textile & Handloom                                                               Exercise 1.2.20
           Shawl Weaving Artisan - Winding and Warping

           Storing warped yarn and ensuring stability

           Objectives : At the end of this exercise you shall be able to
           •  learn how to keep the warped yarn beam safe and in good condition after warping is done, until it is used
            in weaving.

             Requirements

              Tools/Equipment’s/Instruments
             •  Warped beam                        - 1 No.      •  Labels or paper tags            - as reqd.
             •  Plastic sheet or cloth to cover    - as reqd.   •  Trolley or beam stand           - 1 No.
             •  Rope or rubber bands to tie yarn ends  - as reqd.  •  Pen and notebook             - 1 No each.

           PROCEDURE

           Step 1: Check the beam before storage.               •  Use a paper tag or sticker and write

           •  Look at the beam carefully.                                            Table 2
           •  Check these things.                                S.No.         Label              Example
                                Table 1
                                                                   1       Yarn count             30s count
            S.No.     What to check         Yes (or) No            2       No. of yarn ends          400
                    Yarn is wound
              1     properly and evenly                            3       Length of warp        1000 meters

                    No yarn is broken or                           4       Date of warping
              2     loose

                    Beam is not                                    5       Trainee name
              3     damaged                                     •  Check Label is written clearly

                    Beam has a label or                         •  Check Label is fixed on the beam
              4     tag attached
                                                                Step 5: Store Beam in the Right Place
           Step 2: Tie the loose yarn ends                      •  Keep the beam on a rack or trolley, not on the floor.
           •  Take all loose yarns and tie them together gently.  •  Keep in a clean, dry, and cool place.
           •  Use a rubber band or soft rope.
                                                                •  Do not keep it in sunlight, water, or near walls.
           •  This stops yarns from getting tangled.            Safety tips

           Step 3: Cover the beam                               •  Always use help or trolley to move the beam (don’t
           •  Use a clean plastic cover or cotton cloth.           lift it alone).
           •  Cover the beam fully to protect from dust and     •  Never drag the beam on the ground.
              sunlight.                                         •  Wash your hands or wear gloves to keep yarn clean.
           Step 4: Attach a label
           •  Every beam should have a label with important
              details.

           26

| 33 34 35 36 37 38 39 40 41 42 43 |