Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 41 - Shawl Weaving Artisan - TP
P. 41

    TASK 3: Weaver’s knot (Fig 1)

                1  Take the yarn and form a loop at its end.           Fig 1
                2  Take the other end and pass through the loop.
                3  Wrap the working end around the standing part of
                   the loop.
                4  Tuck the working end under itself and pull both ropes
                   to tighten the knot.

                TASK 4: Lark’s head knot (Fig 1)
                1  Take the  two loose ends and fold them over and     Fig 1
                   around the object.
                2  Now take these two loose ends through the loop at
                   the folded end.

                3  Pull the loose ends evenly together to tighten.

                TASK 5 : Half bow knot (Fig 1)

                1  Start with both ends of the tie even, unless you want   Fig 1
                   to tie it to the side.
                2  Make a loop, similar to how you would tie any bow.

                3  Wrap the other end around the loop.
                4  Pull the  other end through until it’s  completely
                   through.
                5  Tighten and adjust as needed

                                Textile & Handloom : Shawl Weaving Artisan (NSQF - 2024) Exercise 1.2.22            29

| 36 37 38 39 40 41 42 43 44 45 46 |