Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 70 - Shawl Weaving Artisan - TP
P. 70

    2  Secondary motion
                                                          Table 1

             S No.             Loom motion                                Name of the motion

               1

               2

           TASK 2: Practice primary motion of the loom

           1  Sit on the loom which is fully operated.
           2  Press the treadles according to design. (Fig 1)    Fig 2

            Fig 1

                                                                4  Now pass the shuttle between the divided warp with
                                                                   the help of picker or hand.(picking motion).fig.

           3  Now the warp yarn is divided into two layers.     5  Then beat the filling thread with the help of reed
              (this gap  between warp yarn is known as  shed).     (beating).
              (Fig 2)
                                                                6  Now change the treadle and repeat the process.

           TASK 3: Secondary motion of the loom

           1  After completing  the primary  motion, stop the    Fig 1
              weaving.
           2  Now open the lock of the warp beam and then cloth
              beam.(in a through shuttle loom) (Fig 1)
           3  Now release the warp from the warp beam (let off
              motion).
           4  Then wind the woven cloth onto the cloth beam.(take
              up motion).
           5  After the let off and take up motion, lock the warp
              beam and cloth beam again.
           6  Now start the weaving with primary motions.

           58             Textile & Handloom : Shawl Weaving Artisan (NSQF - 2024) Exercise 1.5.39

| 65 66 67 68 69 70 71 72 73 74 75 |