Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 34 - Shawl Weaving Artisan - TP
P. 34

    6  Adjust the tension so the yarns stay tight but not too   Fig 6
             stretched while winding. (Fig 5)
            Fig 5

                                                                8  Keep an eye on the threads to ensure they are going
           7  Now Rotate the beam in the clock wise direction. As   on evenly and in the right order.
              shown in Fig 6
                                                                9  Stop when you have transferred the required length
                                                                   of yarns

                                                                10 Tie or secure the yarn ends on the beam.

           22             Textile & Handloom : Shawl Weaving Artisan (NSQF - 2024) Exercise 1.2.17

| 29 30 31 32 33 34 35 36 37 38 39 |