Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 32 - Shawl Weaving Artisan - TP
P. 32

    Textile & Handloom                                                                Exercise 1.2.16

           Shawl Weaving Artisan - Winding and Warping

           Warping on warp beam

           Objectives : At the end of this exercise you shall be able to
           •  prepare warp sheet for weaving process.

             Requirements

              Tools/Equipment’s/Instruments
              •  Measuring tape                  - 1 No.
              •  Scissor small size              - 1 No.

           PROCEDURE

           Winds the yarn on beam

           1  Check the attachment of threads on the beam.      7  Repeat the  steps and prepare 20 meters  length
           2  Now slightly rotate the beam.                        warp. (Fig 2)
           3  Observe the movement of threads through the reed   Fig 2
              and winding on the beam.
           4  Measure the circumference of  the beam by using
              measuring tape.
           5  If the circumference is 1 meter, than the one rotation
              indicates 1 meter length of yarn.
           6  Now do 10 revolution i.e.  10 meter length warp.
              (Fig 1)
           Fig 1

           20

| 27 28 29 30 31 32 33 34 35 36 37 |