Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 85 - Shawl Weaving Artisan - TP
P. 85

    Table 1

                                                                                                          Final
                 Sample code  Appearance         Twist         Ply          Feel        Burn test
                                                                                                      identification
                       1
                       2
                       3
                       4

                C  Identification of fabrics                          2  Feel test
                1  Visual inspection                                  •  Stretch fabric lengthwise and width wise.
                •  Look for weave structure:                          •  Check thickness, flexibility, and softness.

                   -  Plain (over-under)                              3  Yarn pull test
                   -  Twill (diagonal lines)                          •  Unravel a yarn from the edge.
                   -  Satin (smooth surface)                          •  Observe if it pulls  easily  (woven)  or comes  off in
                                                                        loops (knitted).
                   -  Knitted (loops)
                   -  Non-woven (random bonding)                      Observation Table (For trainees to Fill)

                                                                Table 1

                   Sample     Visual appearance         Feel         Stretch     Yarn pull test   Final Identification
                     No
                      1

                      2

                      3
                      4

                                Textile & Handloom : Shawl Weaving Artisan (NSQF - 2024) Exercise 1.6.49            73

| 80 81 82 83 84 85 86 87 88 89 90 |