Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 33 - Shawl Weaving Artisan - TP
P. 33

    Textile & Handloom                                                                Exercise 1.2.17
                Shawl Weaving Artisan - Winding and Warping

                Winding of warp from warping drum

                Objectives : At the end of this exercise you shall be able to
                •  prepare warp beam for weaving process.

                  Requirements

                   Tools/Equipment’s/Instruments
                   •  Warping drum                     - 1 No.        •  Paper sheet                        - as reqd.
                   •  Warp beam                        - 1 No.        •  Thread for lease                   - as reqd.

                PROCEDURE

                1  Set up an empty beam near to the warping drum.     4  Then attach the yarn to the lease  rod which  is
                                                                        attached to the beam (Fig 3)
                2  Take one section of yarn from the warping drum and
                   keep them straight and untangled. (Fig 1)           Fig 3

                  Fig 1

                                                                      5  Likewise attach all the sections to the beam. (Fig 4)

                3  Now Insert lease threads between the warp, so the   Fig 4
                   warp became untangled Fig.2

                 Fig 2

                                                                                                                    21

| 28 29 30 31 32 33 34 35 36 37 38 |